
            ******** README.TXT **********

     VISHAY NOBEL AB, Sweden
     www.vishaynobel.com

     BatchView  version 1.10             2002-11-19


     ENGLISH (for Swedish see below)
     -------------------------------


     This document includes information and 
     instructions on how to get started with BatchView 
     together with Vishay Nobel's instrument TAD 3.


     Table of Contents
     -----------------
     1.     What is BatchView
     2.     Connections
     3.     Menu File
     4.     Menu Tools
     5.     BatchView main window
     6.     Log file format



     1. What is BatchView.
     --------------------
     BatchView is a batching utility program
     that runs under Windows95/98 or Windows NT4. It can be used 
     with Vishay Nobel's instrument TAD 3 with standard batching option.

     The product comes with the following functions:
     - Control the batching in TAD 3 (Start/Stop/Reset/Restart/....)
     - Display of batching status
     - Display/Edit batch data
     - Save batch data in file, Fetch batch data from file
     - Logging of batching events to file
     - Display/Edit/Print accumulated weights  




     2. Connections
     --------------
     BatchView communicates with the connected instrument via a 
     serial port (COM1 - COM4) on the PC. In the normal case this 
     port is a RS232 port, and if the serial ports on the 
     instruments are RS485 ports, the connection has to go 
     through a RS232/RS485 converter. If the PC has a built
     in RS485 port the converter can be omitted.
     The connection could use 2-wire or 4-wire RS485. If 2-wire
     RS485 is used the converter has to have automatic data
     direction control.


     Connection diagram (4 wire RS485)

     -------------|     |---------------|     |---------------
     PC RS232 port|     |  Converter    |     |Vishay Nobel
     COM1 - COM4  |     |  RS485/RS232  |     |Instrument TAD 3
                  |     |               |     |
            (DTE) |     |(DCE)          |     | 
            RS232 |     |RS232    RS485 |     |RS485    
            9p 25p|     |25p 9p       A'|-----|TXD-         
             3  2 |-----| 2   3       B'|-----|TXD+          
             2  3 |-----| 3   2       A |-----|RXD-         
             5  7 |-----| 7   5       B |-----|RXD+        
                  |     |           COM.|-----|COM.  
                  |     |               |     |  
     -------------|     |---------------|     |---------------

     Make sure the converter is jumpered for 4-wire RS485 and
     that the bus is terminated.
     See also the instrument and converter manual for further
     information on how the serial port should be connected.


     Connection diagram (RS232)

     -------------|                           |---------------
     PC RS232 port|                           |Vishay Nobel
     COM1 - COM4  |                           |Instrument TAD 3
                  |                           |
            (DTE) |                           | 
            RS232 |                           |COM 1 RS-232    
            9p 25p|                           |(D-sub, 9 pin)         
             3  2 |---------------------------| 3 (RXD)          
             2  3 |---------------------------| 2 (TXD)         
             5  7 |---------------------------| 5 (COM.)   
                  |                           |  
                  |                           |  
     -------------|                           |---------------




     3. Menu File
     ------------
     Fetch Batch Data from file...
        Fetch batch data from file and send it to the connected TAD 3.

     Save Batch Data in file...
        Save current batch data in a file.



     4. Menu Tools
     -------------
     Accumulated weight...
        Opens an accumulated weight dialog box where all accumulated
        weights are displayed. From this dialog box the accumulated
        weights can be printed on the default printer using the Print
        button.
        An accumulated weight can be edited by double clicking the 
        desired weight (password may be required). Press enter to
        accept the new value or Escape to cancel.
     
     TAD 3 Utils...
        Opens a TAD 3 dialog box where weight and status for the
        connected TAD 3 instrument is displayed. From this dialog
        box it is also possible to perform a number of basic 
        commands as tare, set to zero, set remote operation on/off,....

     Reinitiate
        Reinitiates the BatchView program and reads new data from
        the connected TAD 3. Use this command, or restart the BatchView
        program, as soon you have made any changes in the TAD 3 set-up.

     Set-Up...
        Opens a Settings dialog box (password may be required) from 
        where it is possible to make a number of settings for the
        BatchView program.
        - Language: Possible to select English or Swedish.
        - Change password: Possible to change the Set-up and
          the User password. Entering a blank password will disable
          the password function. The Set-up password is used to enter
          the Set-up menu and User password is used when changing
          batch data and accumulated weights.
        - Log file: Used to select if batching events shall be 
          logged in a file, and if so, to which file.
        - Communication: Used to select the address of the 
          connected TAD 3 and other communication parameters
          (baud rate, parity and communication port).
          NOTE! The instrument address and communication parameters
          must be set equal as in TAD 3.



     5. BatchView main window
     ------------------------
     The main window shows:
        - Instrument name of the connected TAD 3.
        - Gross and net weigh with taring possibilities.
        - The last opened batch data file and information if the batch 
          data in the file and in the instrument differs.
        - Current batch data from TAD 3 that can be edited by double 
          clicking the desired value (password may be required).
          (Press enter to accept the new value or Escape to cancel)
        - Current batch status from TAD 3.
        - Batch number, Batched weight and Total batched weight (for
          current batch) that are updated during batching.

     There are also a number of buttons that can be used to control
     the batching (Start, Stop,...) from the program. Only buttons
     that are active for the moment are enabled, all other buttons
     are disabled. 

     For detailed information about Batching, see TAD 3 Technical Manual.

        

     6. Log file format
     -------------------
     The log file is an ASCII-file where each line is terminated by CRLF.
     Each line is divided into tab-separated fields and each line 
     corresponds to one batching event.
     Following fields are available (from left to right):
       Date, Time, Event number, Event description, 
       Number of batches, Batch size, Batch size unit, Batch number, 
       Activity number, Activity name, Setpoint, Setpoint unit,
       Batched weight (for current activity), Unit for batched weight,
       Subtotal (for current batch), Unit of subtotal, 
       Name (including path) of current batch data file, Remark.

     Where "Event number" 11 - 17 corresponds to standard 
     batching alarm code 01 - 07 (see TAD 3 Technical manual)
     and 1 - 4 corresponds to events as below.
     Event:  1 = Batching started
             2 = Activity ready
             3 = Batch ready
             4 = Batching finished

     Where "Remark" is a text that indicates that the data in current
     batch data file differs from the batch data in the instrument.

     NOTE! All fields will not contain data for all events. 
     Only selected fields will be filled in for each type of event.



     ===================================================================
     ===================================================================



     SVENSKA (for English see above)
     -------------------------------


     Detta dokument innehåller information och
     instruktioner om hur BatchView kan användas
     tillsammans med Vishay Nobel's TAD 3 instrument.


     Innehåll
     --------
     1.     Vad är BatchView
     2.     Anslutningar
     3.     Meny Arkiv
     4.     Meny Verktyg
     5.     BatchView huvudfönster
     6.     Format på loggfil



     1. Vad är BatchView
     -------------------
     BatchView är ett hjälpprogram för dosering som körs 
     under Windows95/98 or Windows NT4. Det kan användas
     tillsammans med Vishay Nobel's TAD 3 instrument
     med standard doseringsoption.

     Följande funktioner ingår i programmet:
     - Styrning av doseringen i TAD 3 (Start/Stopp/Avbryt/Återstart/....)
     - Visning av doseringsstatus
     - Visning/Ändring av doseringsdata
     - Spara doseringsdata i fil, Hämta doseringsdata från fil
     - Registrering av doseringshändelser i fil
     - Visning/Ändring/Utskrift av ackumulerade vikter



     2. Anslutningar
     ---------------
     BatchView kommunicerar med det anslutna instrumentet via en 
     seriell port (COM1 - COM4) på Pc:n. I normala fall är denna 
     port en RS232 port, och om den seriella porten på  
     instrumentet är en RS485 port, måste anslutningen göras 
     genom en RS232/RS485 konverterare. Om Pc:n har en inbyggd RS485
     port kan konverteraren uteslutas.
     Anslutningen kan göras via 2-tråds eller 4-tråds RS485. Om 2-tråds
     RS485 används måste konverteraren ha automatisk omkoppling av
     datariktningen.


     Anslutning (4-tråds RS485)

     -------------|     |---------------|     |---------------
     PC RS232 port|     |  Konverterare |     |Vishay Nobel
     COM1 - COM4  |     |  RS485/RS232  |     |Instrument TAD 3
                  |     |               |     |
            (DTE) |     |(DCE)          |     | 
            RS232 |     |RS232    RS485 |     |RS485    
            9p 25p|     |25p 9p       A'|-----|TXD-         
             3  2 |-----| 2   3       B'|-----|TXD+          
             2  3 |-----| 3   2       A |-----|RXD-         
             5  7 |-----| 7   5       B |-----|RXD+        
                  |     |           COM.|-----|COM.  
                  |     |               |     |  
     -------------|     |---------------|     |---------------

     Kontrollera att konverteraren är byglad för 4-tråd RS485 och
     att dataledningarna är avslutade.
     Se också beskrivningarna för instrumentet och konverteraren
     för mera information om hur anslutningarna skall utföras.


     Anslutning (RS232)

     -------------|                           |---------------
     PC RS232 port|                           |Vishay Nobel
     COM1 - COM4  |                           |Instrument TAD 3
                  |                           |
            (DTE) |                           | 
            RS232 |                           |COM 1 RS-232    
            9p 25p|                           |(D-sub, 9 pin)         
             3  2 |---------------------------| 3 (RXD)          
             2  3 |---------------------------| 2 (TXD)         
             5  7 |---------------------------| 5 (COM.)   
                  |                           |  
                  |                           |  
     -------------|                           |---------------




     3. Meny Arkiv
     -------------
     Hämta doseringsdata från fil...
        Hämta doseringsdata från en fil och skicka dem till 
        det anslutna TAD 3 instrumentet.

     Spara doseringsdata i fil...
        Spara aktuell doseringsdata i en fil.



     4. Meny Verktyg
     ---------------
     Ackumulerad vikt...
        Öppnar ett fönster där alla ackumulerade vikterna visas.
        Från detta fönster kan de ackumulerade vikterna
        skrivas ut på standardskrivaren med knappen "Skriv ut".
        En ackumulerad vikt kan ändras genom att dubbelklicka på den
        önskade vikten (lösenord kan behövas). Tryck retur för att
        acceptera det nya värdet eller Escape för att avbryta.
     
     TAD 3 Hjälpmedel...
        Öppnar ett TAD 3 fönster där vikt och status för det anslutna
        TAD 3 instrumentet visas. Från detta fönster går det också att
        utföra ett antal grundläggande kommandon som tarera,
        nollställa, välja fjärrstyrning till/från,....

     Reinitiera
        Initierar om BatchView programmet och läser in nya data från det
        anslutna TAD 3 instrumentet. Använd detta kommando, eller starta
        om BatchView programmet, om du gjort några ändringar TAD 3 
        instrumentets uppsättning.

     Inställningar...
        Öppnar ett fönster för inställningar (lösenord kan behövas) där 
        det går att göra ett antal inställningar för BatchView programmet.
        - Språk: Möjlighet att välja mellan Engelska eller Svenska.
        - Ändra lösenord: Möjlighet att ändra lösenordet för Inställning
          och Användare. Inmatning av ett blankt lösenord stänger av 
          lösenordsfunktionen. Lösenord för Inställning används för att få
          tillträde till inställningsmenyn och lösenord för Användare 
          används vid ändring av doseringsdata och ackumulerade vikter.
        - Loggfil: Används för att välja om doseringshändelser skall 
          registreras i en fil, och om så är fallet, i vilken fil.
        - Kommunikation: Används för att ange adress på det anslutna TAD 3
          instrumentet och för att ställa in övriga kommunikationsparametrar 
          (överföringshastighet, paritet och kommunikationsport).
          OBS! Instrumentadress och kommunikationsparametrarna måste
          ställas in lika som de i TAD 3 instrumentet.



     5. BatchView huvudfönster
     -------------------------
     Huvudfönstret visar:
        - Instrumentnamnet på ansluten TAD 3.
        - Brutto- och nettovikt med möjlighet till att tarera.
        - Namnet på den senast öppnade doseringsdatafilen och
          information om doseringsdata i filen avviker från
          doseringsdata i instrumentet.
        - Aktuell doseringsdata från TAD 3 som kan ändras genom
          att dubbelklicka på det önskade värdet (lösenord kan behövas).
          (Tryck retur för att acceptera det nya värdet eller Escape för att avbryta)
        - Aktuellt doseringsstatus från TAD 3.
        - Satsnummer, Doserad vikt och Totalt doserad vikt (för 
          aktuell sats) som uppdateras under pågående dosering.

     Det finns också ett antal knappar som kan användas för att styra
     doseringen (Start, Stopp,...) från programmet. Bara knappar
     som är aktiva för tillfället är i funktion, alla övriga knappar är avstängda.

     För detaljerad information angående dosering, se TAD 3 Teknisk handbok.



     6. Format på loggfil
     --------------------
     Loggfilen är en ASCII-file där varje rad avslutas med CRLF.
     Varje rad är indelad i tab-separerade fält och varje rad  
     motsvarar en doseringshändelse.
     Följande fält finns (från vänster till höger):
       Datum, Tid, Händelsenummer, Händelsebeskrivning, 
       Antal satser, Satsstorlek, Enhet på satsstorlek, Satsnummer, 
       Activitetsnummer, Activitetsnamn, Börvärde, Enhet på börvärde,
       Doserad vikt (för aktuell aktivitet), Enhet på doserad vikt,
       Subtotal (för aktuell sats), Enhet på subtotal, 
       Namn (inklusive sökväg) på aktuell doseringsdatafil, Anmärkning.

     Där "Händelsenummer" 11 - 17 motsvarar standard kod för 
     doseringslarm 01 - 07 (se TAD 3 Teknisk handbok) och 1 - 4
     motsvarar händelser enligt nedan.
     Händelse:  1 = Dosering startad
                2 = Aktivitet klar
                3 = Sats klar
                4 = Dosering avslutad

     Där "Anmärkning" är en text som indikerar om data i aktuell
     doseringsdatafil avviker från doseringsdata i instrumentet.

     OBS! Alla fält innehåller inte data för alla händelser.
     Bara vissa fält kommer att innehålla data för varje typ av händelse.





